# USGS 1:25000-scale Quadrangle for Island Of Kosrae, FM 2001

TypeRaster Dataset

Tags There are no tags for this item.

### Summary

    To provide the Kosrae USGS Historical Quadrangle Series (2001) in GIS format (GeoTiff).

### Description

    To provide the Kosrae USGS Historical Quadrangle Series (2001) in GIS format (GeoTiff). The USGS Historical Quadrangle Scanning Project (HQSP) is scanning all scales and all editions of topographic maps published by the U.S. Geological Survey (USGS) since the inception of the topographic mapping program in 1884.

### Credits

    Acknowledgment of the U.S. Geological Survey is expected for products derived from these data.

### Use limitations

    None. However, users should be aware that temporal changes may have occurred since this map was originally produced and that some parts of this data may no longer represent actual surface conditions. Users should not use this data for critical applications without a full awareness of its limitations.

### Extent

There is no extent for this item.

### Scale Range

There is no scale range for this item.

### Topics and Keywords ▼►

Themes or categories of the resourceImagery & Base Maps
Theme keywordsGeoTiff, GeoPDF
  Thesaurus ▼►
    TitleThe National Map Product Format Thesaurus
Theme keywordsHistorical Topographic Maps, Historical Topographic Maps 7.5 x 7.5 Minute Map Series
  Thesaurus ▼►
    TitleThe National Map Collection Thesaurus
Theme keywords7.5 x 7.5 minute
  Thesaurus ▼►
    TitleThe National Map Product Extent Thesaurus
Theme keywordsimageryBaseMapsEarthCover
  Thesaurus ▼►
    TitleISO 19115 Topic Category
Theme keywordsDownloadable Data
  Thesaurus ▼►
    TitleThe National Map Type Thesaurus
Theme keywordsMap
  Thesaurus ▼►
    TitleThe National Map Theme Thesaurus
Place keywordsIsland Of Kosrae (Northeast), Island Of Kosrae (Southeast), Kosrae, Federated States of Micronesia (FSM), U.S. Affiliated Pacific Islands (USAPI), Caroline Islands, Micronesia, Northwestern Pacific, Pacific Ocean
  Thesaurus ▼►
    TitleGeographic Names Information System

### Citation ▼►

TitleUSGS 1:25000-scale Quadrangle for Island Of Kosrae, FM 2001
Alternate titlesUSGS_Topo_NE_462386_2001_25000.tif
Publication date2020-08
Presentation formatsdigital map
FGDC geospatial presentation formatScanned Map in GeoTIFF
Collection titleHistorical Topographic Maps 7.5 x 7.5 Minute Map Series

### Citation Contacts ▼►

Responsible party - originator
  Organization's nameU.S. Geological Survey
Responsible party - publisher
  Organization's nameU.S. Geological Survey
    Contact information ▼►
      Address
        Delivery pointReston, Virginia
Responsible party - distributor
  Organization's nameIsland Research & Education Initiative (iREi)

### Resource Details ▼►

Dataset languagesEnglish (UNITED STATES)
Dataset character setutf8 - 8 bit UCS Transfer Format
Statuscompleted
Spatial representation typegrid
Spatial resolution
  Dataset's scale
    Scale denominator25000
Graphic overview
  File name https://prd-tnm.s3.amazonaws.com/StagedProducts/Maps/HistoricalTopo/2/15091/5050730.jpg
  File descriptionThumbnail JPG image of map
  File typeJPEG
Supplemental information

      The dataset is included in the Digital Atlas of Micronesia, module Kosrae, created by Island Research & Education Initiative (iREi) in collaboration with Water and Environmental Research Institute of the Western Pacific (WERI) at the University of Guam and funding from United States Geological Survey (USGS) under WRRI 104-B Program and FSM Department of Environment, Climate Change & Emergency Management (DECEM).

Processing environmentEsri ArcGIS 10.6
Credits

      Acknowledgment of the U.S. Geological Survey is expected for products derived from these data.

### Extents ▼►

Extent
  Geographic extent
    Bounding rectangle
      West longitude162.883335
      East longitude163.066701
      South latitude5.249379
      North latitude5.383943
Extent
  Description

        publication date

  Temporal extent
    Beginning date2001-01-01
    Ending date2002-01-01
Extent
  Description

        NOTE: Bounding Coordinates identified in FGDC metadata are associated with the GNIS Cell ID; {"gdaId" : 5930051, "cellId" : 395614, "scale" : 25000, "pageWidth" : 29, "pageHeight" : 31.1}

### Resource Points of Contact ▼►

Point of contact - point of contact
  Organization's nameU.S. Geological Survey
    Contact information ▼►
      Phone
        Voice1-888-ASK-USGS (1-888-275-8747)
      Address
        Typephysical
        Delivery point12201 Sunrise Valley Drive
        CityReston
        Administrative areaVirginia
        Postal code20192
        CountryUS
      Hours of service

            Monday through Friday 8:00 AM to 4:00 PM Eastern Time Zone USA

      Contact instructions

            Please visit http://www.usgs.gov/ask/ to contact us.

Point of contact - point of contact
  Organization's nameU.S. Geological Survey
  Individual's nameDrew Decker
  Contact's positionNational Map Liaison
    Contact information ▼►
      Phone
        Voice619-225-6430
      Address
        Delivery point4165 Spruance Road
        CitySan Diego
        Administrative areaCA
        Postal code92101
        e-mail address ddecker@usgs.gov

### Resource Maintenance ▼►

Resource maintenance
  Update frequencynot planned

### Resource Constraints ▼►

Legal constraints
  Limitations of use

        Although these data have been processed successfully on a computer system at the U.S. Geological Survey, no warranty expressed or implied is made regarding the accuracy or utility of the data on any other system or for general or scientific purposes, nor shall the act of distribution constitute any such warranty. This disclaimer applies both to individual use of the data and aggregate use with other data. It is strongly recommended that these data are directly acquired from a U.S. Geological Survey server, and not indirectly through other sources which may have changed the data in some way. It is also strongly recommended that careful attention be paid to the contents of the metadata file associated with these data. The U.S. Geological Survey shall not be held liable for improper or incorrect use of the data described and/or contained herein.

Constraints
  Limitations of use

        None. However, users should be aware that temporal changes may have occurred since this map was originally produced and that some parts of this data may no longer represent actual surface conditions. Users should not use this data for critical applications without a full awareness of its limitations.

### Spatial Reference ▼►

Reference system identifier
  Value32658
  CodespaceEPSG
  Version8.2.6

### Spatial Data Properties ▼►

Georectified Grid ▼►
  Number of dimensions2
  Axis dimensions properties - column (x-axis)
    Dimension size10457
    Resolution
        1.587486 Meter
  Axis dimensions properties - row (y-axis)
    Dimension size11623
    Resolution
        1.587486 Meter
  Cell geometryarea
  Point in pixelcenter
  Transformation parameters are availableYes
  Check points are availableNo
  Corner points
    Point415301.622046 763658.300021
    Point415301.622046 782109.647703
    Point431901.961262 782109.647703
    Point431901.961262 763658.300021
  Center point423601.791654 772883.973862

### Spatial Data Content ▼►

Image Description
  Type of informationthematic classification
  Band information
    DescriptionBand_1
    Maximum value255.000000
    Minimum value0.000000
    Number of bits per value8

### Data Quality ▼►

Scope of quality information ▼►
  Resource leveldataset
Data quality report - Conceptual consistency ▼►
  Data quality measure reference
    Measure description

          This product is a GeoPDF file. GeoPDF is a copyright format with implementation rights held exclusively by TerraGo Technologies. This design is based on use of specific commercial software systems therefore any changes to the software specifications and dependencies will be followed by the USGS and codified in the product standard.

Data quality report - Absolute external positional accuracy ▼►
  dimensionhorizontal
  Data quality measure reference
    Measure description

          The digital GeoPDF version of the historical map was georeferenced with a methodology that preserves, but does not exceed, the accuracy of the original map. The historical map product was compiled to meet National Map Accuracy Standards (NMAS) of the era when the map was originally published.

### Lineage ▼►

Process step ▼►
  When the process occurred2001-01-01
  Description

        Date on Map

Process step ▼►
  When the process occurred2001-01-01
  Description

        Aerial Photo Year

Process step ▼►
  When the process occurred2002-01-01
  Description

        Imprint Year

Process step ▼►
  When the process occurred2013-01-01
  Description

        The GeoPDFs for the scanned Historical Quadrangles are produced using the following steps. Historical Quadrangles are scanned typically at 600 PPI (minimum of 400 PPI). Metadata is collected from the information printed in the map collar. Scanned TIFF images are georeferenced to the original map datum, and reprojected to the original map projection. The final GeoPDF file is generated using TerraGo Publisher for Raster software. To support the use of the GeoPDF file in the U.S. Army Geospatial Center GeoPDF seamless viewing tool, neatline coordinates are added to the GeoPDF header file. Last, an FGDC compliant XML metadata file is generated and attached to the GeoPDF. Note that GeoPDF is a copyrighted format, with implementation rights held exclusively by TerraGo Technologies. Any use of trade, product, or firm names in this publication is for descriptive purposes only and does not imply endorsement by the U.S. Government.

Process step ▼►
  When the process occurred2017-01-10 00:00:00
  Description

        Converted from GeoPDF to GeoTIFF Global Mapper software.

  Process contact - processor
    Organization's nameU.S. Geological Survey
    Individual's nameDrew Decker
    Contact's positionNational Map Liaison
      Contact information ▼►
        Phone
          Voice619-225-6430
        Address
          Delivery point4165 Spruance Road
          CitySan Diego
          Administrative areaCA
          Postal code92101
          e-mail address ddecker@usgs.gov
  Source data ▼►
    Source citation ▼►
      Collection titleHistorical Topographic Maps 7.5 x 7.5 Minute Map Series
Process step ▼►
  When the process occurred2017-07-15 00:00:00
  Description

        Imported xml metadata from original GeoPDF and updated information.

  Process contact - processor
    Organization's nameIsland Research & Education Initiative (iREi)
    Individual's nameMaria Kottermair
    Contact's positionGIS Specialist
      Contact information ▼►
        Address
          e-mail address mariakottermair@gmail.com
Source data ▼►
  Description

        USGS provided the scanned copy of the historical quadrangle.

  Source medium namehardcopy—printing on paper
  Resolution of the source data
    Scale denominator25000
  Source citation ▼►
    TitleOriginal Paper Map
    Alternate titlesmap
    Publication date2001-01-01
    Other citation details

          Island Of Kosrae (Northeast), FM; U.S. Department of the Interior, USGS Scanned Historical Quadrangle Standard, Version 1.0.

    Responsible party - originator
      Organization's nameUSGS
  Extent of the source data
    Description

          publication date

    Temporal extent
      Date and time2001-01-01

### Distribution ▼►

Distributor ▼►
  Contact information - distributor
    Organization's nameU.S. Geological Survey
      Contact information ▼►
        Phone
          Voice1-888-ASK-USGS (1-888-275-8747)
        Address
          Typephysical
          Delivery point12201 Sunrise Valley Drive
          CityReston
          Administrative areaPohnpei
          Postal code20192
          CountryUS
        Hours of service

              Monday through Friday 8:00 AM to 4:00 PM Eastern Time Zone USA

        Contact instructions

              Please visit http://www.usgs.gov/ask/ to contact us.

  Available format
    NameGeoPDF
  Ordering process
    Terms and feesNone
  Transfer options
    Transfer size10.5204
    Online source
      Online location (URL) https://prd-tnm.s3.amazonaws.com/StagedProducts/Maps/HistoricalTopo/2/15091/5050729.pdf
Distributor ▼►
  Contact information - distributor
    Organization's nameIsland Research & Education Initiative (iREi)
      Contact information ▼►
        Address
          Typepostal
          Delivery pointP.O. Box PS 303
          CityPalikir
          Administrative areaPohnpei
          Postal code96941
          CountryFM
          e-mail address irei@islandresearch.org
        Online resource
          Online location (URL)www.islandresearch.org/
  Transfer options
    Online source
      Online location (URL) http://islandatlas.org
      NameDigital Atlas of Micronesia – module Kosrae
      Function performeddownload
Distribution format
  NameRaster Dataset
Transfer options
  Online source
    Online location (URL) https://prd-tnm.s3.amazonaws.com/StagedProducts/Maps/HistoricalTopo/2/15091/5050729.pdf

### References ▼►

Aggregate Information
  Association typelarger work citation
  Aggregate resource name ▼►
    TitleHistorical Topographic Maps 7.5 x 7.5 Minute Map Series
    Publication date2006-01-01
    Responsible party - originator
      Organization's nameU.S. Geological Survey
    Resource location online
      Online location (URL) https://www.sciencebase.gov/catalog/item/4f5543b2e4b018de15819c9d

### Metadata Details ▼►

Metadata languageEnglish (UNITED STATES)
Metadata character setutf8 - 8 bit UCS Transfer Format
Scope of the data described by the metadatadataset
Scope namedataset
Last update2020-08-28
ArcGIS metadata properties
  Metadata formatESRI-ISO

### Metadata Contacts ▼►

Metadata contact - point of contact
  Organization's nameU.S. Geological Survey
    Contact information ▼►
      Phone
        Voice1-888-ASK-USGS (1-888-275-8747)
      Address
        Typephysical
        Delivery point12201 Sunrise Valley Drive
        CityReston
        Administrative areaVirginia
        Postal code20192
        CountryUS
      Hours of service

            Monday through Friday 8:00 AM to 4:00 PM Eastern Time Zone USA

      Contact instructions

            Please visit http://www.usgs.gov/ask/ to contact us.

Metadata contact - processor
  Organization's nameIsland Research & Education Initiative (iREi)
  Individual's nameMaria Kottermair
  Contact's positionGIS Specialist
    Contact information ▼►
      Address
        Type
        e-mail address mariakottermair@gmail.com